**RCM-28 2.0.15 for IRIS-Net Release Notes**

• This firmware update fixes a bug with Dante routing using the RCM-28 firmware supplied with IRIS-Net 4.0

How to use:

1. Delete the firmware that you have currently in the IRIS-Net 4.0 installation folder: RCM28 V2\_0\_15.capfw
2. Copy the attached firmware file RCM28\_2\_0\_15\_id1026\_cap3\_40.capfw into the RCM-28 Firmware Folder of IRIS-Net 4.0
3. Install the newest version of the Firmware Upload Tool, which is included in the IRIS-Net Tools directory
4. Update all Amplifiers with this Firmware: RCM28\_2\_0\_15\_id1026\_cap3\_40.capfw

